**To charge:**

1. Disconnect batteries before plugging in charger.
2. Press *ENTER* once to view charge screen.
3. Press INC / DEC to select charge rate.
4. Connect charge and balance cables to battery.
5. Hold *ENTER* to begin charging.
6. When prompted, press *ENTER* again to confirm cell type.
7. Press *DEC* twice to view charge voltage and current during charge.

**To stop charge, or when complete:**

1. Hold *ENTER*. Screen displays *CHARGER STOPPED.*
2. Press *BACK* to return to charge screen.
3. Disconnect battery before unplugging charger.